STM32F4xxLED

#### STM32F4xx Leds control

Home page | Led control | ADC status bar

This page allows you to control the four LEDs: LED1, LED2, LED3 and LED4 located in the STM324xG-EVAL board. To put on/off
a LED you have to check/uncheck its corresponding checkbox. Then you have to click on "Send" button to submit the new LEDs
configuration. Finally check in the STM324xG-EVAL board that you get the desired LEDs are putted on/off.

STM32 Webserver LEDs Control

LED1
LED2
LED3
LED4

###

###

_______________________________________________________________________________________________________________
All rights reserved © 2013 STMicroelectronics